/*
 * Copyright (c) 2021 The ZMK Contributors
 *
 * SPDX-License-Identifier: MIT
 */

#include <dt-bindings/zmk/matrix_transform.h>

/ {
    chosen {
        zmk,kscan = &kscan0;
        zmk,matrix-transform = &default_transform;
    };

    /*
     * This transform correspondsto the 60% left without macro keypad and 65% right, even this
     * combination of PCBs can have keys in different locations based on configuration.
     */
    default_transform: keymap_transform_0 {
        compatible = "zmk,matrix-transform";
        columns = <13>;
        rows = <4>;
        map = <
RC(0,0) RC(0,1) RC(0,2) RC(0,3) RC(0,4) RC(0,5)      /**/  RC(0,6) RC(0,7) RC(0,8) RC(0,9) RC(0,10) RC(0, 11) RC(0,12)
RC(1,0)   RC(1,1) RC(1,2) RC(1,3) RC(1,4) RC(1,5)    /**/  RC(1,6) RC(1,7) RC(1,8) RC(1,9) RC(1,10) RC(1,12)
RC(2,0)     RC(2,1) RC(2,2) RC(2,3) RC(2,4) RC(2,5)  /**/    RC(2,6) RC(2,8) RC(2,9) RC(2,10) RC(2,11) RC(2,12)
RC(3,0)   RC(3,1) RC(3,2) RC(3,3) RC(3,4)            /**/  RC(3,6)        RC(3,9)  RC(3,10)  RC(3,11)  RC(3,12)
        >;
    };

    kscan0: kscan {
        compatible = "zmk,kscan-gpio-matrix";
        wakeup-source;

        diode-direction = "col2row";
        row-gpios
            = <&pro_micro 21 (GPIO_ACTIVE_HIGH | GPIO_PULL_DOWN)>  // Row A
            , <&pro_micro 6 (GPIO_ACTIVE_HIGH | GPIO_PULL_DOWN)>   // Row B
            , <&pro_micro 7 (GPIO_ACTIVE_HIGH | GPIO_PULL_DOWN)>   // Row C
            , <&pro_micro 8 (GPIO_ACTIVE_HIGH | GPIO_PULL_DOWN)>   // Row D
            ;
    };
};
