peripheral 0 <inf> bt_hci_core: HW Platform: Nordic Semiconductor (0x0002)
peripheral 0 <inf> bt_hci_core: HW Variant: nRF52x (0x0002)
peripheral 0 <inf> bt_hci_core: Firmware: Standard Bluetooth controller (0x00) Version 3.5 Build 0
peripheral 0 <wrn> bt_id: No static addresses stored in controller
peripheral 0 <inf> bt_hci_core: Identity: D1:0B:03:A3:ED:6F (random)
peripheral 0 <inf> bt_hci_core: HCI: version 5.4 (0x0d) revision 0x0000, manufacturer 0x05f1
peripheral 0 <inf> bt_hci_core: LMP: version 5.4 (0x0d) subver 0xffff
peripheral 0 <dbg> zmk: kscan_mock_schedule_next_event_0: delaying next keypress: 5000
peripheral 0 <inf> zmk: Welcome to ZMK!
peripheral 0 <dbg> zmk: security_changed: Security changed: FD:9E:B2:48:47:39 (random) level 2
peripheral 0 <dbg> zmk: split_svc_pos_state_ccc: value 1
peripheral 0 <dbg> zmk: split_svc_select_phys_layout_callback: Selecting physical layout after GATT write of 0
peripheral 0 <dbg> zmk: kscan_mock_work_handler_0: ev 327680000 row 0 column 0 state 0
peripheral 0 <dbg> zmk: kscan_mock_schedule_next_event_0: delaying next keypress: 5000
peripheral 0 <dbg> zmk: zmk_physical_layouts_kscan_process_msgq: Row: 0, col: 0, position: 0, pressed: false
peripheral 0 <dbg> zmk: split_listener:
peripheral 0 <dbg> zmk: kscan_mock_work_handler_0: ev 2475163905 row 1 column 1 state 1
peripheral 0 <dbg> zmk: kscan_mock_schedule_next_event_0: delaying next keypress: 5000
peripheral 0 <dbg> zmk: zmk_physical_layouts_kscan_process_msgq: Row: 1, col: 1, position: 3, pressed: true
peripheral 0 <dbg> zmk: split_listener:
peripheral 0 <dbg> zmk: split_svc_run_behavior: offset 0 len 20
peripheral 0 <dbg> zmk: split_svc_run_behavior: sysreset with params 0 0: pressed? 1
